---
title: "hyd1d - Vignette"
author: "Arnd Weber"
date: "`r Sys.Date()`"
output:
  html_vignette:
    toc: yes
    toc_depth: 3
  html_document:
    toc: yes
    toc_depth: '3'
    df_print: paged
  pdf_document:
    latex_engine: pdflatex
    keep_tex: no
    number_sections: yes
    toc: yes
    toc_depth: 3
    fig_width: 7
    fig_height: 6
    fig_caption: yes
    df_print: kable
    highlight: tango
    includes:
      in_header: latex/header.tex
      before_body: latex/before_body.tex
    pandoc_args: "--biblatex"
bibliography: ../inst/REFERENCES.bib
csl: apa_modified.csl
link-citations: yes
documentclass: scrreprt
classoption:
- a4paper
- twoside
geometry:
- left=3.2cm
- right=3.2cm
- top=2.8cm
- bottom=3cm
- marginparwidth=2cm
- marginparsep=0.3cm
lang: en
linkcolor: blue
urlcolor: blue
citecolor: blue
lof: yes
vignette: |
  %\VignetteIndexEntry{hyd1d - Vignette} 
  %\VignetteEncoding{UTF-8} 
  %\VignetteEngine{knitr::rmarkdown} 
---

```{r setup, include = FALSE}
knitr::opts_chunk$set(
    collapse = TRUE,
    comment = "#>",
    fig.align="center",
    fig.width = 7,
    fig.height = 4, 
    root.dir = "vignettes"
)
```

<!-- Indent in html version TOC
     obtained from: 
     https://stackoverflow.com/questions/46201753/rmarkdown-indentation-of-toc-items-in-html-output
     -->

<script>
$(document).ready(function() {
  $items = $('div#TOC li');
  $items.each(function(idx) {
    num_ul = $(this).parentsUntil('#TOC').length;
    $(this).css({'padding-left': num_ul * 5px, 'box-shadow': none});
  });

});
</script>

<!-- numbering for figures and tables-->
```{r captions, echo = FALSE, error = FALSE, warning = FALSE, message = FALSE, include = FALSE}
library(hyd1d)
library(stringr)
library(yaml)
library(desc)

# set english locale to produce english plot labels
Sys.setlocale(category = "LC_MESSAGES", locale = "en_US.utf8")

# Determine the output format of the document
outputFormat <- knitr::opts_knit$get("rmarkdown.pandoc.to")
if (outputFormat == "html") {
    is_html <- TRUE
} else {
    is_html <- FALSE
}

# Figure and Table Caption Numbering, for HTML do it manually
capTabNo <- 1
capFigNo <- 1

# Function to add the Table Number
capTab <- function(x){
    if(outputFormat == 'html'){
        x <- paste0("**Tab. ", capTabNo, "**: ", x)
        capTabNo <<- capTabNo + 1
    } else if (outputFormat == 'latex'){
        y <- str_replace_all(x, '(^.*)(\\[.*\\])(\\(.*\\))(.*$)', 
                             '\\1\\\\href{\\3}{\\2}\\4')
        y <- gsub("{(", "{", y, fixed = TRUE, useBytes = TRUE)
        y <- gsub("{[", "{", y, fixed = TRUE, useBytes = TRUE)
        y <- gsub(")}", "}", y, fixed = TRUE, useBytes = TRUE)
        y <- gsub("]}", "}", y, fixed = TRUE, useBytes = TRUE)
        x <- gsub("_", "\\_", y, fixed = TRUE, useBytes = TRUE)
    }
    return(x)
}

# Function to add the Figure Number
capFig <- function(x){
    if(outputFormat == 'html'){
        x <- paste0("**Fig. ", capFigNo, "**: ", x)
        capFigNo <<- capFigNo + 1
    } else if (outputFormat == 'latex'){
        y <- str_replace_all(x, '(^.*)(\\[.*\\])(\\(.*\\))(.*$)', 
                             '\\1\\\\href{\\3}{\\2}\\4')
        y <- gsub("{(", "{", y, fixed = TRUE, useBytes = TRUE)
        y <- gsub("{[", "{", y, fixed = TRUE, useBytes = TRUE)
        y <- gsub(")}", "}", y, fixed = TRUE, useBytes = TRUE)
        y <- gsub("]}", "}", y, fixed = TRUE, useBytes = TRUE)
        x <- gsub("_", "\\_", y, fixed = TRUE, useBytes = TRUE)
    }
    return(x)
}

href <- function(x, y) {
    if (outputFormat == 'html') {
        x <- paste0("[", x, "](", y, ")")
    } else if (outputFormat == 'latex') {
        x <- paste0("\\href{", y, "}{", x, "}")
    }
    return(x)
}

bf <- function(x) {
    if (outputFormat == 'html') {
        x <- paste0("**", x, "**")
    } else if (outputFormat == 'latex') {
        x <- paste0("\\textbf{", x, "}")
    }
    return(x)
}
# Function to simplify linking to references/rd
lrd <- function(x, y) {
    # standard url
    url <- "https://hyd1d.bafg.de"
    
    # url from DESCRIPTION file
    if (file.exists("DESCRIPTION")) {
        url_desc <- description$new("DESCRIPTION")$get_urls()[1]
    }
    
    # url from pkgdown/_pkgdown.yml
    pwd <- Sys.getenv("PWD")
    if (pwd != "") {
        if (file.exists(paste0(pwd, "/pkgdown/_pkgdown.yml"))) {
            url_pkgdown <- yaml.load_file(
                paste0(pwd, "/pkgdown/_pkgdown.yml"))$url
        }
    }
    
    if (exists("url_desc")) {
        url <- url_desc
        if (exists("url_pkgdown")) {
            url <- url_pkgdown
        }
    }
    
    # outputformat latex
    if (knitr::is_latex_output()) {
        if (missing(y)) {
            if (endsWith(x, "()")) {
                x1 <- gsub("()", "", x, fixed = TRUE)
                str <- paste0("[", x, "](", url, "/reference/", x1, ".html)")
            } else {
                str <- paste0("[", x, "](", url, "/reference/", x, ".html)")
            }
        } else {
            str <- paste0("[", x, "](", url, "/reference/", y, ")")
        }
        return(str)
    }
    
    # outputformat html
    if (missing(y)) {
        if (endsWith(x, "()")) {
            # x1 <- gsub("()", "", x, fixed = TRUE)
            str <- paste0("`", x, "`")
        } else {
            str <- paste0("<code>[", x, "](", url, "/reference/", x, ".html)</",
                          "code>")
        }
    } else {
        str <- paste0("<code>[", x, "](", url, "/reference/", y, ")</code>")
    }
    
    return(str)
}
```

<BR>

# Purpose

**hyd1d** is an R package that provides an S4-class and several functions to 
compute 1-dimensional water levels along the German federal waterways Elbe and 
Rhine.

<BR>

# Use

## Installation

The package **hyd1d** is available from CRAN. To install it run:

```{r install_cran, eval = FALSE}
install.packages("hyd1d")
```

To install the recent developmental version from opencode.de execute the
following commands: 

```{r install_git, eval = FALSE}
install.packages("pak")
library(pak)
pak::pak("git::https://gitlab.opencode.de/bafg-bund/hyd1d.git")
```

Afterwards **hyd1d** can be loaded like every other R package with the following 
command: 

```{r library, eval = TRUE, echo = TRUE, error = FALSE, warning = FALSE, message = FALSE}
library(hyd1d)
```

## S4-class WaterLevelDataFrame

All water level computations with **hyd1d** are based on the S4-class
`r lrd("WaterLevelDataFrame", "WaterLevelDataFrame-class.html")`. To compute
water levels with one of the
`r lrd("waterLevel...()", "index.html#section-waterlevel-functions")`-functions,
a `r lrd("WaterLevelDataFrame", "WaterLevelDataFrame-class.html")`
has to be initialized with the homonymous `r lrd("WaterLevelDataFrame()")`-function: 

```{r wldf, eval = TRUE}
wldf <- WaterLevelDataFrame(river   = "Elbe",
                            time    = as.POSIXct("2016-12-21"),
                            station = seq(257, 262, 0.1))
```

The required information to initialize a
`r lrd("WaterLevelDataFrame", "WaterLevelDataFrame-class.html")` are
the function arguments `river`, `time` and at least one of the two possible
station arguments (`station` or `station_int`). With this information an object
of class `r lrd("WaterLevelDataFrame", "WaterLevelDataFrame-class.html")` can be
created, which has the following structure:

```{r structure, eval = TRUE}
str(wldf)
summary(wldf)
```

The actual water level information is stored in the S4-slot `.Data`, which is in
fact a `data.frame` with the columns `station`, `station_int` and `w`. The
columns `station` and `station_int` contain a stationing information, which
corresponds to the official stationing of the German Waterways and Shipping Administration
(Wasserstraßen- und Schifffahrtsverwaltung (WSV)). The stationing information is
duplicated to enable database joins with GIS data through the `integer`-type
column `station_int`. The column `w` contains the actual
water level in the height reference system DHHN92 (1992 German height reference
system), but is usually empty after initialization and gets filled
throught the application of one of the
`r lrd("waterLevel...()", "index.html#section-waterlevel-functions")`-functions.

For the application of
`r lrd("waterLevel...()", "index.html#section-waterlevel-functions")`-functions
information stored in the S4-slots `river` and where appropriate `time` is
essential. They enable a distinct localization of the stationing along the
rivers Elbe and Rhine and a determination of the time of water level
computation. The other slots of an object of class
`r lrd("WaterLevelDataFrame", "WaterLevelDataFrame-class.html")` are filled
during the water level computation and contain partial results needed to
visualize the results (`gauging_station`) or serve information purposes (
`gauging_stations_missing`, `comment`).

# Computation of water levels

## waterLevel

The most advanced function to interpolate 
[FLYS3](https://www.bafg.de/DE/5_Informiert/1_Portale_Dienste/FLYS/flys_node.html)
water levels [@bundesanstalt_fur_gewasserkunde_flys_2013; @bundesanstalt_fur_gewasserkunde_flys_2016] with local gauging
data is implemented in the `r lrd("waterLevel()")`-function. This function uses
package-internal gauging data from the dataset `r lrd("df.gauging_data")`, which
contains daily-averaged gauging data since 1960-01-01. Therefore
`r lrd("waterLevel()")` can be applied for the time period  between 1960-01-01
and yesterday.

After the [initialization](hyd1d.html#s4-class-waterleveldataframe) of
a `r lrd("WaterLevelDataFrame", "WaterLevelDataFrame-class.html")` the
application is very simple:

```{r waterlevel, eval = TRUE}
wldf <- waterLevel(wldf)
summary(wldf)
```

And if you want to visualize the results using `r lrd("plotShiny()")` the additional
argument `shiny = TRUE` has to be used. Thereby the columns `section`,
`weight_x` and `weight_y` get created in the `.Data`-Slot, which are required
for visualization.

```{r figure1, fig.show = 'asis', fig.cap = capFig("Interpolated water level, computation-relevant stationary [FLYS3](https://www.bafg.de/DE/5_Informiert/1_Portale_Dienste/FLYS/flys_node.html) water levels (**0.5MQ**, **a** and **0.75MQ**) and gauge height as of 2016-12-21 at River Elbe between Rosslau and Dessau."), eval = TRUE}
wldf <- waterLevel(wldf, shiny = TRUE)
summary(wldf)

xlim_min <- 257
xlim_max <- 263
{
    plotShiny(wldf, TRUE, TRUE, TRUE, xlim = c(xlim_min, xlim_max),
              xlab = "river station (km)",
              ylab = "elevation (m a.s.l. (DHHN92))")
    legend("topright", 
           col = c("darkblue", "darkblue", "darkblue", "red", "black"), 
           pch = c(21, NA, NA, NA, NA), 
           pt.bg = c("darkblue", NA, NA, NA, NA), 
           pt.cex = c(1, NA, NA, NA, NA), 
           lty = c(0, 0, 1, 1, 1), 
           lwd = c(0, 0, 1, 0.6, 0.6), 
           legend = c("gauge height", "gauge weight", "waterLevel", 
                      "upper FLYS w.l.", "lower FLYS w.l."), 
           text.col = c(1, "darkblue", 1, 1, 1), 
           cex = 0.7, bty = "n")
}
```

## waterLevelPegelonline

The way how the `r lrd("waterLevelPegelonline()")`-function
computes a water level is equivalent to the `r lrd("waterLevel()")`-function.
Just the data source of the gauging data is different, since it does not use
package-internal data, but online data provided by
<https://pegelonline.wsv.de/gast/start> [@wsv_pegelonline_2018]. Because data
provided by [PEGELONLINE](https://pegelonline.wsv.de/gast/start) are only
available for the past 30 days, the application of this function is limited to
recent time periods, but with a high temporal resolution.

```{r figure2, fig.show = 'asis', fig.cap = capFig(paste0("Interpolated water level, computation-relevant stationary [FLYS3](https://www.bafg.de/DE/5_Informiert/1_Portale_Dienste/FLYS/flys_node.html) water levels (**0.5MQ**, **a** and **0.75MQ**) and gauge height as of ", strftime(Sys.time() - 3600, format = "%Y-%m-%d %H:%M")," at River Elbe between Rosslau and Dessau.")), eval = hyd1d:::.pegelonline_status()}
# one hour ago
time <- as.POSIXct(Sys.time() - 3600)

# initialize a WaterLevelDataFrame
wldf <- WaterLevelDataFrame(river   = "Elbe",
                            time    = time,
                            station = seq(257, 262, 0.1))

# compute w
wldf <- waterLevelPegelonline(wldf, shiny = TRUE)
summary(wldf)

# and plot the results
{
    plotShiny(wldf, TRUE, TRUE, TRUE, xlim = c(xlim_min, xlim_max),
              xlab = "river station (km)",
              ylab = "elevation (m a.s.l. (DHHN92))")
    legend("topright", 
           col = c("darkblue", "darkblue", "darkblue", "red", "black"), 
           pch = c(21, NA, NA, NA, NA), 
           pt.bg = c("darkblue", NA, NA, NA, NA), 
           pt.cex = c(1, NA, NA, NA, NA), 
           lty = c(0, 0, 1, 1, 1), 
           lwd = c(0, 0, 1, 0.6, 0.6), 
           legend = c("gauge height", "gauge weight", "waterLevel", 
                      "upper FLYS w.l.", "lower FLYS w.l."), 
           text.col = c(1, "darkblue", 1, 1, 1), 
           cex = 0.7, bty = "n")
}

```

## waterLevelFlood1 & waterLevelFlood2

To compare the newly developed functions `r lrd("waterLevel()")` and
`r lrd("waterLevelPegelonline()")` to existing computation methods,
the functions `r lrd("waterLevelFlood1()")` and `r lrd("waterLevelFlood2()")`
have been implemented. These functions compute water levels according to the
Flood1- and Flood2-methods of the modelling environment
[INFORM](https://www.bafg.de/DE/3_Beraet/4_Exp_oekologie/OekoModelle/oekomodelle_node.html#vt-sprg-3)
[@rosenzweig_inform_2011]. They either shift the reference water level **MQ**
vertically, so that it intersects with the gauge height at a selected reference
gauging station, or linearly interpolate water levels with neighboring gauging
stations.

```{r figure3-prep}
wldf <- WaterLevelDataFrame(river   = "Elbe",
                            time    = as.POSIXct("2016-12-21"),
                            station = seq(257, 262, 0.1))

wldf1 <- waterLevelFlood1(wldf, "ROSSLAU", shiny = TRUE)
summary(wldf1)

wldf2 <- waterLevelFlood1(wldf, "DESSAU", shiny = TRUE)
summary(wldf2)

wldf3 <- waterLevelFlood2(wldf)
summary(wldf3)
```

```{r figure3, fig.show = 'asis', fig.cap = capFig("Water levels computed according to the Flood1-method with the reference gauges Rosslau (wldf1) and Dessau (wldf2) and the Flood2-method as of 2016-12-21 at River Elbe between Rosslau and Dessau."), eval = TRUE, echo = FALSE}
df.gs2 <- getGaugingStations(wldf2)

{
    plotShiny(wldf1, FALSE, FALSE, FALSE, xlim = c(xlim_min, xlim_max),
              xlab = "river station (km)",
              ylab = "elevation (m a.s.l. (DHHN92))")
    lines(wldf2$station, wldf2$w, col = "darkblue", lty = 2)
    lines(wldf3$station, wldf3$w, col = "red", lty = 2)
    abline(v = df.gs2$km_qps, lty = 3, lwd = 0.5)
    points(df.gs2$km_qps, df.gs2$wl, pch=21, col="darkblue", bg="darkblue")
    hyd1d:::.boxed.labels(df.gs2$km_qps, 55.4, df.gs2$gauging_station,
                          bg="white", srt = 90, border = FALSE, xpad = 4,
                          ypad = 0.7, cex = 0.7)
    legend("topright", 
           col = c("darkblue", "darkblue", "darkblue", "red"), 
           pch = c(21, NA, NA, NA), 
           pt.bg = c("darkblue", NA, NA, NA), 
           pt.cex = c(1, NA, NA, NA), 
           lty = c(0, 1, 2, 2), 
           lwd = c(0, 1, 1, 1), 
           legend = c("gauge height", "wldf1", "wldf2", "wldf3"), 
           cex = 0.7, bty = "n")
}
```

## waterLevelFlys3InterpolateY

To compare the newly developed functions `r lrd("waterLevel()")` and
`r lrd("waterLevelPegelonline", "waterLevel.html")` to existing computation
methods of
[FLYS3](https://www.bafg.de/DE/5_Informiert/1_Portale_Dienste/FLYS/flys_node.html),
the function `r lrd("waterLevelFlys3InterpolateY()")` has been implemented. This
function computes a water level according to the method implemented in the
W-INFO-module of [FLYS3](https://www.bafg.de/DE/5_Informiert/1_Portale_Dienste/FLYS/flys_node.html).
This function determines the relative position of the gauge height at a
reference gauge to the two surrounding [FLYS3](https://www.bafg.de/DE/5_Informiert/1_Portale_Dienste/FLYS/flys_node.html)
water levels and uses this weight for a longitudinal interpolation between both
water levels.

```{r figure4-prep}
wldf <- waterLevelFlys3InterpolateY(wldf, "ROSSLAU", shiny = TRUE)
summary(wldf)
```

```{r figure4, fig.show = 'asis', fig.cap = capFig("Water levels according to [FLYS3](https://www.bafg.de/DE/5_Informiert/1_Portale_Dienste/FLYS/flys_node.html) with the reference gauge Rosslau as of 2016-12-21 at River Elbe between Rosslau and Dessau."), eval = TRUE, echo = FALSE}
{
    plotShiny(wldf, TRUE, TRUE, TRUE, xlim = c(xlim_min, xlim_max),
              xlab = "river station (km)",
              ylab = "elevation (m a.s.l. (DHHN92))")
    abline(v = df.gs2$km_qps, lty = 3, lwd = 0.5)
    points(df.gs2$km_qps, df.gs2$wl, pch=21, col="darkblue", bg="darkblue")
    hyd1d:::.boxed.labels(df.gs2$km_qps, 55.4, df.gs2$gauging_station,
                          bg="white", srt = 90, border = FALSE, xpad = 4,
                          ypad = 0.7, cex = 0.7)
    legend("topright", 
           col = c("darkblue", "darkblue", "darkblue", "red", "black"), 
           pch = c(21, NA, NA, NA, NA), 
           pt.bg = c("darkblue", NA, NA, NA, NA), 
           pt.cex = c(1, NA, NA, NA, NA), 
           lty = c(0, 0, 1, 1, 1), 
           lwd = c(0, 0, 1, 0.6, 0.6), 
           legend = c("gauge height", "gauge weight", "waterLevel", 
                      "upper FLYS w.l.", "lower FLYS w.l."), 
           text.col = c(1, "darkblue", 1, 1, 1), 
           cex = 0.7, bty = "n")
}
```

## waterLevelFlys3...

All other `waterLevelFlys3...()`-functions (`r lrd("waterLevelFlys3()")`,
`r lrd("waterLevelFlys3Seq()")` and `r lrd("waterLevelFlys3InterpolateX()")`)
serve exclusively for the preparation and querying of stationary
[FLYS3](https://www.bafg.de/DE/5_Informiert/1_Portale_Dienste/FLYS/flys_node.html)
water levels. They can be used to extract water levels from the dataset 
`r lrd("df.flys")`
and interpolate the water levels linearly along the x-axis, but without
modifying the dataset contents. These functionalities are needed for **all**
`r lrd("waterLevel...()", "index.html#section-waterlevel-functions")`-functions
described in this vignette and are mentioned here for completeness.

<BR>

# Products

## waterLevel

The `r lrd("waterLevel()")` function is the central function of the package
**hyd1d**. To apply it only three input parameters, that are needed to
initialize a `r lrd("WaterLevelDataFrame", "WaterLevelDataFrame-class.html")`,
are required. That predestines this function to embed it into an interactive
Shiny Application:

\begin{center}
\url{https://shiny.bafg.de/waterlevel/}
\end{center}

``` {r link_waterlevel, eval = is_html, echo = FALSE, results = 'asis'}
cat('<p style="text-align: center;"><a href="https://shiny.bafg.de/waterlevel/" target="_blank">https://shiny.bafg.de/waterlevel/</a></p>')
```

```{r figure20, echo = FALSE, fig.cap = capFig(paste0("Screenshot of the ", href("waterLevel-ShinyApp", "https://shiny.bafg.de/waterlevel/"), " with the interpolated water level, caomputationrevelvant stationary ", href("FLYS3", "https://www.bafg.de/DE/5_Informiert/1_Portale_Dienste/FLYS/flys_node.html"), "-waterlevels (", bf("0.5MQ"), ", ", bf("a"), " and ", bf("0.75MQ"), ") and gauge heights at 2016-12-21 at the River Elbe between Rosslau and Dessau, Germany.")), fig.show = 'asis', out.width = "100%", results = 'asis'}
knitr::include_graphics('screenshot_waterLevel.png')
```

## waterLevelPegelonline

The same is true for the function `r lrd("waterLevelPegelonline()", "waterLevel.html")`. 
Since this function queries gauging data through the internet and not from 
package-internal datasets, the resulting shiny application is well suited to
generate up-to-date water level information.

\begin{center}
\url{https://shiny.bafg.de/waterlevelpegelonline/}
\end{center}

``` {r link_waterlevelpegelonline, eval = is_html, echo = FALSE, results = 'asis'}
cat('<p style="text-align: center;"><a href="https://shiny.bafg.de/waterlevelpegelonline/" target="_blank">https://shiny.bafg.de/waterlevelpegelonline/</a></p>')
```

```{r figure21, echo = FALSE, fig.cap = capFig(paste0("Screenshot of the ", href("waterLevelPegelonline-ShinyApp", "https://shiny.bafg.de/waterlevelpegelonline/"), " with the interpolated water level, computationrevelvant stationary ", href("FLYS3", "https://www.bafg.de/DE/5_Informiert/1_Portale_Dienste/FLYS/flys_node.html"), "-waterlevels (", bf("a"), ", ", bf("0.75MQ"), " and ", bf("0.5MQ"), ") and gauge heights at 2018-04-13 11:00 a.m. at the River Elbe between Rosslau and Dessau, Germany.")), fig.show = 'asis', out.width = "100%"}
knitr::include_graphics('screenshot_waterLevelPegelonline.png')
```

## hydflood (flood extents and durations)

The R package **hydflood** enables the modelling of flood extents and durations
through an extrapolation of water levels computed along the river axis with
functions provided within R package **hyd1d** to cross section areas and GIS
operations comparing these water levels to digital elevation models. Daily flood
extents can be aggregated over longer time periods to flood durations
(e.g. days/year). More details to this method can be found on the corresponding
package documentation of **hydflood**:

\begin{center}
\url{https://hydflood.bafg.de}
\end{center}

``` {r link_hydflood, eval = is_html, echo = FALSE, results = 'asis'}
cat('<p style="text-align: center;"><a href="https://hydflood.bafg.de" target="_blank">https://hydflood.bafg.de</a></p>')
```

<BR>

# References

