DDT                     Apply demean, detrend, cosine taper
IRISSeismic-deprecated
                        Deprecated Functions in Package 'IRISSeismic'
IRISSeismic-package     Classes and methods for seismic data analysis
IrisClient-class        Class '"IrisClient"'
McNamaraBins            McNamara Binning
McNamaraPSD             Power Spectral Density
STALTA                  STA/LTA
Stream-class            Class '"Stream"'
Trace-class             Class '"Trace"'
TraceHeader-class       Class '"TraceHeader"'
assignQuality           Assign a quality code to a 'Stream' or 'Trace'
butterworth             Apply Butterworth filter
crossSpectrum           Cross-Spectral Analysis
envelope                Envelope of a seismic signal
eventWindow             Return a portion of a trace surrounding an
                        event.
getAvailability         Retrieve Channel metadata from EarthScope
getChannel              Retrieve Channel metadata from EarthScope
getDataAvailability     Retrieve miniseed trace extents from EarthScope
getDataselect           Retrieve seismic data from EarthScope
getDistaz               Retrieve great circle distance information from
                        EarthScope
getEvalresp             Retrieve instrument response information from
                        EarthScope
getEvent                Retrieve seismic event information from the
                        USGS NEIC
getGaps                 Gap analysis
getNetwork              Retrieve Network metadata from EarthScope
getRotation             Retrieve rotated seismic data from EarthScope
getSNCL                 Retrieve seismic data from EarthScope
getStation              Retrieve Station metadata from EarthScope
getTimeseries           Retrieve seismic data from EarthScope
getTraveltime           Retrieve seismic traveltime information from
                        EarthScope
getUnavailability       Retrieve Channel metadata from EarthScope
getUpDownTimes          Determine times when a channel starts/stops
                        collecting data
hilbert                 Hilbert of a seismic signal
hilbertFFT              Hilbert FFT
length                  Length, Max, Mean, Median, Min and Standard
                        Deviation
mergeTraces             Merge multiple traces into a single trace
mergeUpDownTimes        Determine overlaps in two sets of upDownTimes.
miniseed2Stream         Convert miniSEED bytes to 'Stream' object
multiplyBy              Multiplication by a constant
noiseMatrix2PdfMatrix   Convert matrix of PSDs to matrix of Probability
                        Density Functions
noiseModels             Generate NHNM and NLNM noise models
psdDF2NoiseMatrix       Apply instrument correction to PSDs
psdList                 Apply McNamara PSD algorithm to a seismic
                        signal
psdList2NoiseMatrix     Apply instrument correction to PSDs
psdPlot                 Generate plots from a set of PSDs
psdStatistics           Return statistics for a set of PSDs
readMiniseedFile        Convert miniSEED file to 'Stream' object
rms                     Root Mean Square and RMS Variance
rotate2D                Rotate horizontal components of a seismic
                        signal
slice                   Slice a section out of a 'Trace' or 'Stream'
surfaceDistance         Earth surface distance between two points
transferFunctionSpectra
                        function to retrieve response values to use for
                        input to the
                        IRISMustangMetrics::transferFunctionMetric
triggerOnset            Event onset triggering
unHistogram             Histogram to Vector
